{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["DB","Filtri","Output"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"DB","index":0,"n_rows":2193,"n_cols":10,"rows_kept":2193,"cut":false,"hidden":true,"merged":[]}
["Material","UNI EN"," AWS","Wire (mm)","Gas","Process","Type","Power Source","Special Function","Firmware version"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.14"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.14"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.12"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.12"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.1"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.13"]
["Rutil flux core wire","T 46 4 P M21 1 H5 ","E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.2"]
["Rutil flux core wire","T 46 4 P M21 1 H5 ","E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.2"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.1.13"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.12"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.12"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.4"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.4"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405d/505d","X","1.0.4"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.5"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.6"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.10"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.10"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.11"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.10"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.10"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405d/505d","DSI","1.0.11"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.14"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.14"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.14"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.8"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.8"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405d/505d","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.6"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.4"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.7"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.1"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.8"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.4"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.11"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.11"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.11"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405d/505d","K-deep / DSI","1.0.11"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.5"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.9"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.14"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405d/505d","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.13"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.14"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.14"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.12"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.12"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.6"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.1"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.13"]
["Rutil flux core wire","T 46 4 P M21 1 H5 ","E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.2"]
["Rutil flux core wire","T 46 4 P M21 1 H5 ","E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.2"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.1.13"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.12"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.12"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.4"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.4"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 405dms/505dms","X","1.0.4"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.5"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.10"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.10"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.11"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.10"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.10"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 405dms/505dms","DSI","1.0.11"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.14"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.14"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.14"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.8"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.8"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 405dms/505dms","X","1.0.4"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.6"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.4"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.7"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.1"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.8"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.4"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.11"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.11"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.11"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 405dms/505dms","K-deep / DSI","1.0.11"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.5"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.9"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.14"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 405dms/505dms","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 ","E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 ","E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 5000","DSI","1.0"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 5000","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 5000","K-deep / DSI","1.0"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 5000","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 4000K","DSI","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 4000K","K-deep / DSI","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.4"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.4"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 4000K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 4000K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Power MIX","HC/Power Root","Power Pulse 3200K","DSI","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Power Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 3200K","K-deep / DSI","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.4"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.4"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Micro Pulse 225d","X","1.1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Micro Pulse 225d","X","1.1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.1"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.1"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.1"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Pulse 225d","X","1.1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.1"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Pulse 225d","X","1.1.0"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.1.0"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Micro Pulse 225d","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Micro Mag 225","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Mag 225","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Mag 225","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Mag 225","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Micro Mag 225","X","1.0"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.1"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.1"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Micro Mag 225","X","1.0"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Micro Mag 225","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403/503MSR","X","2.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.7"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","2.1"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.7"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.7"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.9"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.1"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.1"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403/503 MSR","X","1.8"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.8"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.8"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403/503 MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.9"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.9"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.9"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.1"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.1"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer pulse 403/503MSR","X","1.8"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.7"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.8"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.8"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer pulse 403/503MSR","X","2.1"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer pulse 403/503MSR","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.7"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","2.1"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.7"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.7"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.9"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.1"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.1"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer 403MKS","X","1.8"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.8"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.8"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","2.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer pulse 403MKS","X","2.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.9"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.9"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.9"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.9"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.9"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.1"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.1"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.0"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 403MKS","X","1.8"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.7"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.8"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.8"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 403MKS","X","2.1"]
["Copper","CuSi3","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Copper","CuSi3","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 403MKS","X","1.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power pulse 322","X","7.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","23 12","ER 309 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","14343-A-G299","ER 312 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","Z 19 9 Ti","ER 321",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Inox flux core wire","T19 9 LRC3","E 308 LT0-1",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Nichel Alloy","S Ni 6625","ER NiCrMo3",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Stellite","TCo1","ER CCoCr-C",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1.2,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I3 30% Ar+70%He","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Power pulse 322","X","7.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power pulse 322","X","7.2"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power pulse 322","X","7.2"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Copper","CuAl8","ER CuAl-A1",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power pulse 322","X","7.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Power Pulse 402/502","X","9.3"]
["Steel","G69 4 M21 Mn3Ni1CrMo","ER110S-G",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","23 12","ER 309 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","14343-A-G299","ER 312 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","Z 19 9 Ti","ER 321",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Inox flux core wire","T19 9 LRC3","E 308 LT0-1",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Nichel Alloy","S Ni 6625","ER NiCrMo3",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Nichel Alloy","S Ni 6625","ER NiCrMo3",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Nichel Alloy","S Ni 6022","ER NiCrMo-10",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Stellite","TCo1","ER CCoCr-C",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I3 80% Ar+20%He","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I3 70% Ar+30%He","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.6,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","High Speed","Power Pulse 402/502","X","9.3"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Power Pulse 402/502","X","9.3"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuAl8","ERCuAl-A1",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuAl8","ERCuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuAl8","ERCuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Copper","CuAl8","ERCuAl-A1",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Power Pulse 402/502","X","9.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlMg5","ER 5356",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlSi5","ER 4043",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Copper","CuAl8","ERCuAl-A1",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Copper","CuAl8","ERCuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Copper","CuAl8","ERCuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MKS","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlMg5","ER 5356",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlSi5","ER 4043",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Copper","CuAl8","ERCuAl-A1",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Copper","CuAl8","ERCuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Copper","CuAl8","ERCuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer 321MSR","X","Gen.2.0/Mot.2.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","14343-A-G299","ER 312 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","Z 19 9 Ti","ER 321",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Inox flux core wire","T19 9 LRC3","E 308 LT0-1",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Nichel Alloy","S Ni 6625","ER NiCrMo3",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Stellite","TCo1","ER CCoCr-C",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I3 30% Ar+70%He","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuAl8","ER CuAl-A1",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MKS","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Control","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","14343-A-G299","ER 312 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","Z 19 9 Ti","ER 321",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Inox flux core wire","T19 9 LRC3","E 308 LT0-1",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Duplex flux core wire","T 22 9 3 NLP M21 2","E2209 T1",1,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Nichel Alloy","S Ni 6625","ER NiCrMo3",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Nichel Alloy","S Ni 6082","NiCrMn3Nb",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Stellite","TCo1","ER CCoCr-C",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"M12-ArHeC-35/2","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I3 30% Ar+70%He","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Control","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuAl8","ER CuAl-A1",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 321MSR","X","Gen.5.6/Mot.5.2"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Stainless Steel","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Nichel Alloy","S Ni 6625","ER NiCrMo3",1,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlMg5","ER/R 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlMg5","ER/R 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlMg5","ER/R 5356",1,"I1 100% Ar","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlMg5","ER/R 5356",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","High Speed","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuAl8","ERCuAl-A1",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuAl8","ERCuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuAl8","ERCuAl-A1",0.8,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Copper","CuAl8","ERCuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Micropulse 302MFK","X","Gen.4.4/Mot.4.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.4,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Aluminium","AlMg5","ER 5356",0.8,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Aluminium","AlSi5","ER 4043",0.8,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Copper","CuSi3 ","ER CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Copper","CuSi3 ","ER CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Copper","CuSi3 ","ER CuSi-A",1.2,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Copper","CuAl8","ERCuAl-A1",0.8,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Copper","CuAl8","ERCuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]
["Copper","CuAl8","ERCuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","MicroMAG 302MFK","X","1.6"]

{"sheet":"Filtri","index":1,"n_rows":31,"n_cols":19,"rows_kept":31,"cut":false,"hidden":true,"merged":[]}
["Material",null,"UNI EN",null," AWS",null,"Wire (mm)",null,"Gas",null,"Process",null,"Type",null,"Power Source",null,"Special Function",null,"Firmware version"]
["Aluminium",null,"18 8 Mn",null,"-",null,0.8,null,"C1 100%CO2",null,"Power MIX",null,"HC/Power Root",null,"Micro Mag 225",null,"DSI",null,"1.0.1"]
["Basic flux core wire",null,"19 12 3",null,"CuSi-A",null,0.9,null,"I1 100% Ar",null,"Sinergico pulsato",null,"High Control",null,"Micro Mag 302MFK",null,"K-deep / DSI",null,"1.0.10"]
["Copper",null,"19 9",null,"E2209-17",null,1,null,"M12 Ar+2,5%CO1",null,"Sinergico short/spray",null,"Power Focus",null,"Micro Pulse 225d",null,"X",null,"1.0.11"]
["Duplex",null,"19 9 Nb",null,"E70C-6M H4",null,1.2,null,"M12 Ar+2,5%CO2",null,null,null,"Power Root",null,"Micro Pulse 302MFK",null,null,null,"1.0.12"]
["Duplex flux core wire",null,"23 12",null,"E70T-5M-J H4",null,1.4,null,"M20 Ar+8-10%CO2",null,null,null,"Standard",null,"Pioneer 3200K",null,null,null,"1.0.13"]
["Inox",null,"AlMg4,5Mn",null,"E71T-11",null,1.6,null,"M21 Ar+18-20%CO2",null,null,null,"Cladding",null,"Pioneer 321MKS",null,null,null,"1.0.14"]
["Metal cored",null,"AlMg5",null,"E71T-1M-J H4",null,null,null,"no gas",null,null,null,"High Speed",null,"Pioneer 321MSR",null,null,null,"1.0.2"]
["Nichel Alloy",null,"AlSi5",null,"ER 307 L",null,null,null,"M12-ArHeC-35/2",null,null,null,null,null,"Pioneer 4000K",null,null,null,"1.0.3"]
["Rutil flux core wire",null,"CuAl8",null,"ER 308 L",null,null,null,"I3 30% Ar+70%He",null,null,null,null,null,"Pioneer 403/503 MSR",null,null,null,"1.0.4"]
["self-shielded",null,"CuSi3",null,"ER 309 L",null,null,null,null,null,null,null,null,null,"Pioneer 403MKS",null,null,null,"1.0.5"]
["Steel",null,"CuSn",null,"ER 316 L",null,null,null,null,null,null,null,null,null,"Pioneer Pulse 3200K",null,null,null,"1.0.6"]
["SuperDuplex",null,"E 22 9 3 NLR",null,"ER 347",null,null,null,null,null,null,null,null,null,"Pioneer Pulse 321MKS",null,null,null,"1.0.7"]
["Stellite",null,"G 13 4 ",null,"ER 5183",null,null,null,null,null,null,null,null,null,"Pioneer Pulse 321MSR",null,null,null,"1.0.8"]
["Inox flux core wire",null,"G 19 12 3 Nb",null,"ER 4043",null,null,null,null,null,null,null,null,null,"Pioneer Pulse 4000K",null,null,null,"1.0.9"]
[null,null,"G 22 9 3 NL",null,"ER 410 NiMo",null,null,null,null,null,null,null,null,null,"Pioneer Pulse 403/503MSR",null,null,null,"1.1.0"]
[null,null,"G 25 9 4 NL",null,"ER 5356",null,null,null,null,null,null,null,null,null,"Pioneer Pulse 403MKS",null,null,null,"1.1.1"]
[null,null,"G3/4 Si1",null,"ER 70 S-6",null,null,null,null,null,null,null,null,null,"Power Pulse 3200K",null,null,null,"1.1.13"]
[null,null,"GZ 21 33 MnNb",null,"ER Cu",null,null,null,null,null,null,null,null,null,"Power pulse 322",null,null,null,"1.1.2"]
[null,null,"NiCrMo3",null,"ER CuAl-A1",null,null,null,null,null,null,null,null,null,"Power Pulse 4000K"]
[null,null,"T 46 4 P M21 1 H5 ",null,"ER2209",null,null,null,null,null,null,null,null,null,"Power Pulse 402/502"]
[null,null,"T 46 6 B M21 3 H5",null,"ER2594",null,null,null,null,null,null,null,null,null,"Power Pulse 405d/505d"]
[null,null,"T 46 6 M M21 1 H5",null,"ER318",null,null,null,null,null,null,null,null,null,"Power Pulse 405dms/505dms"]
[null,null,"T 49 Z T 11",null,"S Ni 6625"]
[null,null,"14343-A-G299",null,"ER 312 L"]
[null,null,"Z 19 9 Ti",null,"ER 321"]
[null,null,"T19 9 LRC3",null,"E 308 LT0-1"]
[null,null,"T 22 9 3 NLP M21 2",null,"E2209 T1"]
[null,null,"S Ni 6625",null,"ER NiCrMo3"]
[null,null,"S Ni 6082",null,"NiCrMn3Nb"]
[null,null,"TCo1",null,"ER CCoCr-C"]

{"sheet":"Output","index":2,"n_rows":131,"n_cols":10,"rows_kept":131,"cut":false,"hidden":false,"merged":[]}
["Enter your filters"]
["Power Source","Pioneer Pulse 3200K"]
["Material","UNI EN"," AWS","Wire (mm)","Gas","Process","Type","Power Source","Special Function","Firmware version"]
[null,null,null,null,null,null,null,{"$f":"B2","v":"Pioneer Pulse 3200K"}]
[]
["Material","UNI EN"," AWS","Wire (mm)","Gas","Process","Type","Power Source","Special Function","Firmware version"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"C1 100%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.4"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.8,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",0.9,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.4,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.6,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Steel","G3/4 Si1","ER 70 S-6",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Metal cored","T 46 6 M M21 1 H5","E70C-6M H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Rutil flux core wire","T 46 4 P M21 1 H5 "," E71T-1M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Basic flux core wire","T 46 6 B M21 3 H5","E70T-5M-J H4",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["self-shielded","T 49 Z T 11","E71T-11",0.9,"no gas","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","18 8 Mn","ER 307 L",1.2,"M12 Ar+2,5%CO1","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Root","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347 ",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9","ER 308 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","23 12","ER 309 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","23 12","ER 309 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",0.9,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 12 3","ER 316 L",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 19 12 3 Nb","ER318",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","19 9 Nb","ER 347",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","G 13 4 ","ER 410 NiMo",1.2,"M20 Ar+8-10%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",0.8,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.4"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex","G 22 9 3 NL","ER2209",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Duplex flux core wire","E 22 9 3 NLR","E2209-17",1.2,"M21 Ar+18-20%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Power Focus","Pioneer Pulse 3200K","X","1.0.3"]
["SuperDuplex","G 25 9 4 NL","ER2594",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Inox","GZ 21 33 MnNb","-",1.2,"M12 Ar+2,5%CO2","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Nichel Alloy","NiCrMo3","S Ni 6625",1.2,"M12 Ar+2,5%CO2","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg5","ER 5356",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlSi5","ER 4043",1.6,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Aluminium","AlMg4,5Mn","ER 5183",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",0.8,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSi3","CuSi-A",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico short/spray","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuAl8","ER CuAl-A1",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]
["Copper","CuSn","ER Cu",1,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.4"]
["Copper","CuSn","ER Cu",1.2,"I1 100% Ar","Sinergico pulsato","Standard","Pioneer Pulse 3200K","X","1.0.3"]